{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"List1","index":0,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[[2,4,2,7]]}
[]
[]
[{"$nulls":4},"Ceny na eshopu"]
["Číslo položky","Název položky","PM","DIVIZE","DEK","PRO-DOMA","IZOMAT","TRADIX"]
[4410050166,"KGEM trubka DN 110x1000mm (76/5016)","Pavlík","VTP",107.42,125.2,107.74,106.36]
[4410050178,"KGEM trubka DN 125x2000mm (60/2160)","Pavlík","VTP",222.1,245.68,233.43,232.73]
[6001138503,"Plastová jímka Smart 5000l - 11.5000.0000","Souček","VTP",22220.93,"nemá",22313,"nemá"]
[4410100014,"FF-Drän DN100 oheb.drenáž.trubka z PVC-U žlutá 50m","Pavlík","VTP",26.5,28.8,34.24,"nemá"]
[1211100604,"Lapač střešních splavenin spodní DN 110 - černá","Souček","VTP",201.64,197.52,338.09,226.12]
[4440005870,"BEST skruž SR-F 1000x1000","Pavlík","VTP",2349.6,2670,2523,2250.41]
[8500038120,"Zemnící pás FEZN 30x4mm,1kg=1,05m (25kg/bal)","Holeček","ELEKTRO",42.66,54.66,50.91,67.599999999999994]
[8500197960,"Korugovaná trubka ohebná pr.40mm ČERVENÁ (50m)","Holeček","ELEKTRO",13.64,18.3,"nemá",21.57]
[8500197880,"Korugovaná trubka ohebná pr.110mm ČERVENÁ (50m)","Holeček","ELEKTRO",39.03,57.34,50.45,67.36]
[8500022363,"Kabel CYKY-J  3x1,5 RE (50m/bal)","Bareš","ELEKTRO",15.2,17.66,17.32,"nemá"]
[8500022423,"Kabel CYKY-J  3x2,5 RE (50m/bal)","Bareš","ELEKTRO",26.44,29.08,27.57,"nemá"]
[4502000120,"EMOS Prodl.kabel PVC 3x1,5mm oranž 1zás spojka; 20m","Bareš","ELEKTRO",648.1,636.9,893.07,663.39]
[4502000220,"EMOS Prodl.kabel buben PVC 1,5mm 4zás IP20; 25m","Bareš","ELEKTRO",972.52,1047.3499999999999,1510.47,858.68]
[4502000240,"EMOS Prodl.kabel buben PVC 1,5mm 4zás IP20; 50m","Bareš","ELEKTRO",1714.66,1734.19,2511,1602.48]
[8500048060,"Instal.kabel UTP Solarix CAT5E PVC 305m/box","Bareš","ELEKTRO",7.11,9.82,"nemá","nemá"]
[8500195890,"FENIX Rohož topná LDTS 160/1,3m2;0,5x2,6m;210W","Bareš","ELEKTRO",1011.66,1253.18,"nemá","nemá"]
[2480205002,"plech Cu 0,55x2000x1000","Bartošová","STRECHY","nemá",3732.07,"nemá","nemá"]
[2480101015,"plech FeZn 0,55x2000x1000","Bartošová","STRECHY",369.6,404.92,"nemá","nemá"]
[1230501030,"TONDACH Stodo 12 -základní A ČR","Majer","STRECHY",49.26,55.01,60.75,82.07]
[1225500011,"BRAMAC CL PP základní taška 1/1 EČ","Majer","STRECHY",38.08,37.5,48.47,46.2]
[3020200172,"lať 4x6/4m impreg.","Makovický","STRECHY",92.91,82.2,"nemá",115.04]
[3820106140,"Palubka SMRK A/B klasik \"C\" 15x121x4m, 8ks/bal SECA","Makovický","STRECHY",1050.55,956.79,"nemá","nemá"]
[2090062211,"Velux okno GLU 0061 MK06","Banýr","STRECHY",8576.36,8887.27,8672.7199999999993,8672.73]
[3010488200,"OSB KRONO 3 18x2500x625 N-4PD (39ks/p)","Makovický","STRECHY",399.61,"nemá",337.41,312.07]
[4582336216,"Máčené rukavice ARDON®PETRAX 10/XL - s prodejní etiketou - okrové","Novák","NARADI",46.58,"nemá","nemá",45.37]
[4592331637,"Plynové topidlo BLP 17 M  - 22510","Liška","NARADI",3950.4,4041.99,4167,"nemá"]
[4502043560,"Kolečko stavební bantam 60L - 139210","Jakovec","NARADI",1237.55,1233.1400000000001,1247,1279.3399999999999]
[3290101934,"FME190 -  elektrické míchadlo STANLEY FATMAX","Liška","NARADI",2313.0100000000002,2305.7800000000002,2296.6999999999998,2558.6799999999998]
[3247205251,"DWE398 QS- Pila Alligator 1700W (duté cihly 20)","Liška","NARADI",8262.7999999999993,8176.35,8263.65,9601.65]
[3630041500,"Sádrokartonová deska RB 12,5mm, hr.PRO (1250/2000mm)","Veirauch","DEKTON",175.07,177.98,175.08,210.17]
[2365100218,"Ceresit CT 80 - 25kg","Zušťák","DEKTON",187.2,187.2,"nemá",213.22]
[3610047692,"HET Klasik - 40kg, int","Buťa","DEKTON",1205.5999999999999,1205.5999999999999,"nemá","nemá"]
[1620185410,"Baumit Nivello Quattro - 25kg","Pokorná","DEKTON",312,296.39999999999998,296.39999999999998,353.64]
[2120800010,"Pouzdro NORMA standard tl. 100mm ZDIVO - 800/1970","Beneš","DEKTON",8095.8,8096.28,8096.28,9054.5499999999993]
[2235102290,"Mamut glue High tack 290 ml bílá","Piekarová","DEKTON",133.05000000000001,123.14,139.91999999999999,159.34]
[4480000028,"Port. směsný cement CEM II/B-M 32,5 R (V-LL), (25kg/bal)","Matěna","STAVIVA",102.96,101.57,102.96,111.07]
["4400821284    ","POROTHERM Cihla 30 Profi Dryfix P10 24,7/30/24,9","Hořák","STAVIVA",64.05,63.28,64.37,70.91]
["4400900900    ","YTONG Klasik 100 příčkovka P2-500 100x249x599","Šebek","STAVIVA",60.8,60.8,56,65.62]
["4400871660    ","BEST ZTRACENÉ BEDNĚNÍ 30 250 přírodní","Dobeš","STAVIVA",56.8,56.8,56.8,"nemá"]
["4400990100    ","Kari sítě KH 30 (100x100 drát 6,0) 3x2","Matěna","STAVIVA",456.2,660.37,464.14,680.99]
[1443002340,"ISOVER DOMO PLUS 100mm (10,08m2/bal)","Marek","IZOLACE",74.67,79.75,78.3,89.92]
[1443000730,"ISOVER UNIROL PROFI 100mm (5,4m2/bal)","Marek","IZOLACE",141.63,145.75,144.38,173.22]
[1460107738,"NatuRoll Pro 100mm (9,24m2/role)","Marek","IZOLACE",73.89,73.89,72.25,94.05]
[1460403140,"EPS 70F 100mm 500x1000 DEK ISOVER (2,5m2/bal)","Telk","IZOLACE",122.5,134.4,126,138.68]
[1420361120,"XPS DEK 300kPa 100mm (FIBRAN ETICS GF I) 3m2/bal","Telk","IZOLACE",279.64999999999998,315.52999999999997,286,307.55]
[1420361120,"XPS DEK 300kPa 100mm (FIBRAN ETICS GF I) 3m2/bal","Telk","IZOLACE","nemá",315.52999999999997,286,"nemá"]
[1020101302,"FATRAFOL 810 t1 tm.šedá 1,5mm š.1,30m (26m2/role)","Matička","IZOLACE","nemá","nemá","nemá","nemá"]
[2640222020,"DEKDREN N8 (P) nop.fólie, v.nopu 8mm, š. 2m (40m2/bal.)","Matička","IZOLACE",21.9,22.23,"nemá",31.29]
[1010301460,"SKLODEK 40 SPECIAL MINERAL (role/7,5m2)","Jekel","IZOLACE",142.80000000000001,"nemá","nemá","nemá"]
[1010984704,"CharBIT ELAST G S40 HQ (role/7,5m2)","Jekel","IZOLACE","nemá",142.04,"nemá",150.96]
[1010201155,"BARUPLAN TOP G S4 mineral (role/7,5m2)","Jekel","IZOLACE","nemá","nemá","nemá","nemá"]
[1010101510,"ASPA BIT V S35 (role/10m2)","Jekel","IZOLACE",64.5,"nemá","nemá","nemá"]
[1010984710,"CharBIT V60 S35 (role/10m2)","Jekel","IZOLACE","nemá",76.14,78.02,80.849999999999994]
[1010101540,"BITUBITAGIT PE V60 S35 (role/10m2)","Jekel","IZOLACE","nemá","nemá","nemá","nemá"]
[]
["Vypracovala:","Fraňková Petra"]
["Dne","2024-09-16"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}