{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"List1","index":0,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[[2,4,2,7]]}
[]
[]
[{"$nulls":4},"Ceny na eshopu"]
["Číslo položky","Název položky","PM","DIVIZE","DEK","PRO-DOMA","IZOMAT","TRADIX"]
[4410050166,"KGEM trubka DN 110x1000mm (76/5016)","Pavlík","VTP",107.42,125.2,107.74,106.36]
[4410050178,"KGEM trubka DN 125x2000mm (60/2160)","Pavlík","VTP",222.1,245.68,233.43,232.73]
[6001138503,"Plastová jímka Smart 5000l - 11.5000.0000","Pavlík","VTP",22308.91,"nemá",22313,"nemá"]
[4410100014,"FF-Drän DN100 oheb.drenáž.trubka z PVC-U žlutá 50m","Pavlík","VTP",24.7,39.06,34.24,"nemá"]
[1211100604,"Lapač střešních splavenin spodní DN 110 - černá","Pavlík","VTP",189,229.26,338.09,226.12]
[4440005870,"BEST skruž SR-F 1000x1000","Pavlík","VTP",2349.6,2670,2523,2250.41]
[8500038120,"Zemnící pás FEZN 30x4mm,1kg=1,05m (25kg/bal)","Holeček","ELEKTRO",41.28,71.58,50.91,58.6]
[8500197960,"Korugovaná trubka ohebná pr.40mm ČERVENÁ (50m)","Holeček","ELEKTRO",14,18.3,"nemá",18.02]
[8500197880,"Korugovaná trubka ohebná pr.110mm ČERVENÁ (50m)","Holeček","ELEKTRO",40.06,57.34,50.45,56.2]
[8500022363,"Kabel CYKY-J  3x1,5 RE (50m/bal)","Bareš","ELEKTRO",18.45,17.66,17.32,"nemá"]
[8500022423,"Kabel CYKY-J  3x2,5 RE (50m/bal)","Bareš","ELEKTRO",29.7,29.08,27.57,"nemá"]
[4502000120,"EMOS Prodl.kabel PVC 3x1,5mm oranž 1zás spojka; 20m","Bareš","ELEKTRO",605.80999999999995,577.69000000000005,893.07,628.51]
[4502000220,"EMOS Prodl.kabel buben PVC 1,5mm 4zás IP20; 25m","Bareš","ELEKTRO",825.61,1166.19,1510.47,959.2]
[4502000240,"EMOS Prodl.kabel buben PVC 1,5mm 4zás IP20; 50m","Bareš","ELEKTRO",1557.17,1970.09,2511,1710.74]
[8500048060,"Instal.kabel UTP Solarix CAT5E PVC 305m/box","Bareš","ELEKTRO",7.11,9.82,"nemá","nemá"]
[8500195890,"FENIX Rohož topná LDTS 160/1,3m2;0,5x2,6m;210W","Bareš","ELEKTRO",1011.66,1253.18,"nemá","nemá"]
[2480205002,"plech Cu 0,55x2000x1000","Bartošová","STRECHY","nemá",3222.75,"nemá","nemá"]
[2480101015,"plech FeZn 0,55x2000x1000","Bartošová","STRECHY",369.6,429.01,"nemá","nemá"]
[1230501030,"TONDACH Stodo 12 -základní A ČR","Majer","STRECHY",50.9,55.01,60.75,53.39]
[1225500011,"BRAMAC CL PP základní taška 1/1 EČ","Majer","STRECHY",38.08,37.5,48.47,40.409999999999997]
[3020200172,"lať 4x6/4m impreg.","Makovický","STRECHY",92.91,82.2,"nemá",80]
[3820106140,"Palubka SMRK A/B klasik \"C\" 15x121x4m, 8ks/bal SECA","Makovický","STRECHY",720,956.79,"nemá","nemá"]
[2090067477,"Velux okno GLU 0061 MK06","Banýr","STRECHY",8576.36,8887.27,8672.7199999999993,"nemá"]
[3010488200,"OSB KRONO 3 18x2500x625 N-4PD (39ks/p)","Banýr","STRECHY",377.27,"nemá",337.41,287.27]
[4582336216,"Máčené rukavice ARDON®PETRAX 10/XL - s prodejní etiketou - okrové","Hloušek","NARADI",46.58,"nemá","nemá",45.37]
[4592331637,"Plynové topidlo BLP 17 M  - 22510","Žák","NARADI",3950.4,4041.99,4167,"nemá"]
[4502043560,"Kolečko stavební bantam 60L - 139210","Jakovec","NARADI",1156.1199999999999,1233.1400000000001,1247,1185.1199999999999]
[3290101934,"FME190 -  elektrické míchadlo STANLEY FATMAX","Liška","NARADI",2352.63,2478.5100000000002,2478.52,2558.6799999999998]
[3247205251,"DWE398 QS- Pila Alligator 1700W (duté cihly 20)","Liška","NARADI",8262.09,8266.44,8263.65,11268.6]
[3630041500,"Sádrokartonová deska RB 12,5mm, hr.PRO (1250/2000mm)","Veirauch","DEKTON",175.07,"na poptání",175.07,160.16999999999999]
[2365100218,"Ceresit CT 80 - 25kg","Zušťák","DEKTON",187.2,187.2,"nemá",239.17]
[3610047692,"HET Klasik - 40kg, int","Melka","DEKTON",1205.5999999999999,1205.5999999999999,"nemá","nemá"]
[1620185410,"Baumit Nivello Quattro - 25kg","Pokorná","DEKTON",312,288.43,296.39999999999998,301.57]
[2120800010,"Pouzdro NORMA standard tl. 100mm ZDIVO - 800/1970","Beneš","DEKTON",8095.8,8096.28,9161.58,9586.7800000000007]
[2235102290,"Mamut glue High tack 290 ml bílá","Piekarová","DEKTON",133.05000000000001,123.14,139.91999999999999,145.12]
[4480000028,"Port. směsný cement CEM II/B-M 32,5 R (V-LL), (25kg/bal)","Matěna","STAVIVA",102.96,101.57,102.96,127.52]
["4400821284    ","POROTHERM Cihla 30 Profi Dryfix P10 24,7/30/24,9","Hořák","STAVIVA",56.73,63.28,65.459999999999994,74.209999999999994]
["4400900900    ","YTONG Klasik 100 příčkovka P2-500 100x249x599","Šebek","STAVIVA",56,60.8,62.4,65.62]
["4400871660    ","BEST ZTRACENÉ BEDNĚNÍ 30 250 přírodní","Obrtel","STAVIVA",56.8,56.8,56.8,"nemá"]
["4400990100    ","Kari sítě KH 30 (100x100 drát 6,0) 3x2","Matěna","STAVIVA",641.14,660.37,640.86,640]
[1443002340,"ISOVER DOMO PLUS 100mm (10,08m2/bal)","Kracík","IZOLACE",75,78.3,78.3,145.04]
[1443000730,"ISOVER UNIROL PROFI 100mm (5,4m2/bal)","Kracík","IZOLACE",143.72,145.75,144.38,275.04000000000002]
[1460107738,"NatuRoll Pro 100mm (9,24m2/role)","Kracík","IZOLACE",72.08,68.97,72.25,80.66]
[1460403140,"EPS 70F 100mm 500x1000 DEK ISOVER (2,5m2/bal)","Telk","IZOLACE",122.01,122.32,125.8,122.48]
[1420361120,"XPS DEK 300kPa 100mm (FIBRAN ETICS GF I) 3m2/bal","Telk","IZOLACE",279.64999999999998,315.54000000000002,293.8,440]
[1420361120,"XPS DEK 300kPa 100mm (FIBRAN ETICS GF I) 3m2/bal","Telk","IZOLACE","nemá",315.54000000000002,293.8,"nemá"]
[1020101302,"FATRAFOL 810 t1 tm.šedá 1,5mm š.1,30m (26m2/role)","Matička","IZOLACE","nemá","nemá","nemá","nemá"]
[2640222020,"DEKDREN N8 (P) nop.fólie, v.nopu 8mm, š. 2m (40m2/bal.)","Matička","IZOLACE",20.7,22.23,"nemá",31.29]
[1010301460,"SKLODEK 40 SPECIAL MINERAL (role/7,5m2)","Jekel","IZOLACE",142.80000000000001,"nemá","nemá","nemá"]
[1010984704,"CharBIT ELAST G S40 HQ (role/7,5m2)","Jekel","IZOLACE","nemá",146.78,"nemá",196.03]
[1010201155,"BARUPLAN TOP G S4 mineral (role/7,5m2)","Jekel","IZOLACE","nemá","nemá","nemá","nemá"]
[1010101510,"ASPA BIT V S35 (role/10m2)","Jekel","IZOLACE",64.5,"nemá","nemá","nemá"]
[1010984710,"CharBIT V60 S35 (role/10m2)","Jekel","IZOLACE","nemá",73.319999999999993,78.02,105.04]
[1010101540,"BITUBITAGIT PE V60 S35 (role/10m2)","Jekel","IZOLACE","nemá","nemá","nemá","nemá"]
[]
["Vypracovala:","Fraňková Petra"]
["Dne","2024-05-27"]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}